<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<library>
<packages>
<package name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
</package>
<package name="HLK-PM01">
</package>
<package name="SG053-SZ">
</package>
<package name="MH-MINI-360">
</package>
<package name="CR1632-THRU">
</package>
<package name="CR1632-SMD">
</package>
<package name="TSR-1">
<description>TSR-1
Series DC/DC Converter</description>
</package>
</packages>
<symbols>
<symbol name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="HLK-PM01">
<pin name="AC1" direction="in"/>
<pin name="AC2" direction="in"/>
<pin name="VO+" direction="pwr"/>
<pin name="VO-" direction="pwr"/>
</symbol>
<symbol name="SG053-SZ">
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="+OUT"/>
<pin name="-OUT"/>
</symbol>
<symbol name="MH-MINI-360">
<pin name="-IN" direction="pwr"/>
<pin name="+IN" direction="pwr"/>
<pin name="+OUT" direction="pwr"/>
<pin name="-OUT" direction="pwr"/>
</symbol>
<symbol name="CR1632BAT">
<description>CR1632 battery holder - thruhole</description>
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="TSR1-2433">
<description>TSR 1-2433
3.3v switching regulator</description>
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="+3V3" direction="pwr"/>
</symbol>
<symbol name="TSR1-2450">
<description>TSR 1-2450
5.0v switching regulator</description>
<pin name="IN" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-DOWN-LM2596"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-DOWN-LM2596">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HLK-PM01">
<description>HI-LINK Ultra-compact power module HLK-PM01&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Meet UL, CE requirements&lt;/li&gt;
&lt;li&gt;Ultra-thin, ultra-small&lt;/li&gt;
&lt;li&gt;All voltage input (AC: 90 ~ 264V)&lt;/li&gt;
&lt;li&gt;Low ripple and low noise&lt;/li&gt;
&lt;li&gt;Output overload and short circuit protection&lt;/li&gt;
&lt;li&gt;High efficiency, high power density&lt;/li&gt;
&lt;li&gt;The product is designed to meet the requirements of EMC and Safety Test&lt;/li&gt;
&lt;li&gt;Low power consumption, environmental protection, no-load loss &lt;0.1W&lt;/li&gt;
&lt;li&gt;100% load aging and testing&lt;/li&gt;</description>
<gates>
<gate name="G$1" symbol="HLK-PM01"/>
</gates>
<devices>
<device name="" package="HLK-PM01">
<connects>
<connect gate="G$1" pin="AC1" pad="P$1"/>
<connect gate="G$1" pin="AC2" pad="P$2"/>
<connect gate="G$1" pin="VO+" pad="P$4"/>
<connect gate="G$1" pin="VO-" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SG053-SZ">
<gates>
<gate name="G$1" symbol="SG053-SZ"/>
</gates>
<devices>
<device name="" package="SG053-SZ">
<connects>
<connect gate="G$1" pin="+IN" pad="P$3 P$4"/>
<connect gate="G$1" pin="+OUT" pad="P$5 P$6"/>
<connect gate="G$1" pin="-IN" pad="P$1 P$2"/>
<connect gate="G$1" pin="-OUT" pad="P$7 P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MH-MINI-360">
<gates>
<gate name="G$1" symbol="MH-MINI-360"/>
</gates>
<devices>
<device name="MINI-360" package="MH-MINI-360">
<connects>
<connect gate="G$1" pin="+IN" pad="P$2"/>
<connect gate="G$1" pin="+OUT" pad="P$3"/>
<connect gate="G$1" pin="-IN" pad="P$1"/>
<connect gate="G$1" pin="-OUT" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CR1632" uservalue="yes">
<description>CR1632 battery holder by Keystone Technologies model 3013</description>
<gates>
<gate name="&lt;NAME" symbol="CR1632BAT"/>
</gates>
<devices>
<device name="CR1632-THP" package="CR1632-THRU">
<connects>
<connect gate="&lt;NAME" pin="P$1" pad="P$1 P$2" route="any"/>
<connect gate="&lt;NAME" pin="P$2" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR1632-SMD" package="CR1632-SMD">
<connects>
<connect gate="&lt;NAME" pin="P$1" pad="P$1 P$2"/>
<connect gate="&lt;NAME" pin="P$2" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSR1-2433">
<description>Traco Power TSR 1-2433
3.3v switching regulator</description>
<gates>
<gate name="G$1" symbol="TSR1-2433"/>
</gates>
<devices>
<device name="" package="TSR-1">
<connects>
<connect gate="G$1" pin="+3V3" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSR1-2450">
<description>Traco Power TSR 1-2450
5.0v switching regulator</description>
<gates>
<gate name="G$1" symbol="TSR1-2450"/>
</gates>
<devices>
<device name="" package="TSR-1">
<connects>
<connect gate="G$1" pin="+5V" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
